Control card settings and database settings realted to LS-DYNA implicit analyses
  guidelines
250425, Ansys 
================================================================================
control_cards_arc.key           Control card settings for use of the arc
                                 length method, for nonlnear postbuckling analysis
control_cards_linear.key        Control card settngs for linear static
                                 analysis
control_cards_nonlin.key        Control cards settings for non-linear static
                                  analysis
control_cards_nonlin_R15.key    Control cards settings for non-linear static
                                  analysis with ParMETIS (ORDER=3) and Mixed
                                  Precision (ISINGLE=1). Can be used from R15.0.2
control_database.k              Control cards settings and database cards for 
                                 non-linear transient explicit analysis. 

control_thermal_steady.key      Additional control cards for steady state thermal
                                  analyses. One of the above control card files may
                                  also be required.
control_thermal_transient.key   Additional control cards for transient thermal
                                  analyses. One of the above control card files may
                                  also be required.

database_cards_dynamic.key      Database cards w. output requests for dynamic
                                  (NOTE: time in ms) analyses
database_cards_static.key       Database cards w. output requsets for static
                                   analyses. Very high frequency output!

database_cards_expl.key         Database cards for explicit analyses. Output intervall
                                 controlled by parameter DBPARU. Must be defined by
                                 the user.
